1,Raw Read Error Rate,6,97,91,OK,00000A0D0480,0,Enabled

3,Spin Up Time,0,100,100,OK (Always passing),000000000000,0,Enabled

4,Start/Stop Count,20,100,100,OK,000000000094,0,Enabled

5,Reallocated Sectors Count,36,100,100,OK,000000000000,0,Enabled

7,Seek Error Rate,30,100,253,OK,000000073927,0,Enabled

9,Power On Time Count,0,100,100,OK (Always passing),000000000156,0,Enabled

10,Spin Retry Count,97,100,100,OK,000000000000,0,Enabled

12,Drive Power Cycle Count,20,100,100,OK,000000000300,0,Enabled

183,SATA Downshift Count,0,100,100,OK (Always passing),000000000000,0,Enabled

184,End-to-End Error Count,99,99,99,Advisory: Usage limit exceeded,000000000001,0,Enabled

187,Reported Uncorrectable Errors,0,1,1,OK (Always passing),0000000006BE,0,Enabled

188,Command Timeout,0,100,98,OK (Always passing),0005000500A0,0,Enabled

189,High Fly Writes,0,100,100,OK (Always passing),000000000000,0,Enabled

190,Airflow Temperature,45,59,55,OK,0000291A0029,0,Enabled

194,Disk Temperature,0,41,45,OK (Always passing),001600000029,0,Enabled

195,Hardware ECC Recovered,0,55,40,OK (Always passing),00000A0D0480,0,Enabled

197,Current Pending Sector Count,0,100,97,OK (Always passing),000000000000,-67,Enabled

198,Off-Line Uncorrectable Sector Count,0,100,97,OK (Always passing),000000000000,-67,Enabled

199,Ultra ATA CRC Error Count,0,200,200,OK (Always passing),000000000000,0,Enabled

240,Head Flying Hours,0,100,253,OK (Always passing),D12D00000015,0,Enabled

241,Total LBA Written,0,100,253,OK (Always passing),0000DBADF6B4,0,Enabled

242,Total LBA Read,0,100,253,OK (Always passing),000013D07D62,0,Enabled